Acid/Metal Separation
The Scanacon ModuFlex or MiniFlex acid-Metal separation system (APU) allows for continuous production in acid-metal finishing processes. By continuously removing dissolved metal contaminants, it enables near indefinite reuse of the finishing solution, reducing acid purchases and waste volumes. The system operates in series with a process filtration apparatus and returns a purified solution with limited acid loss (5% to 15%) for reuse. Only water is needed for regeneration, and the waste product is a weakly acidic solution that can be easily neutralized. With over 25 years of experience and a modular design that allows for expansion and redundancy, Scanacon is the world leader in acid-Metal separation equipment.
Stainless Steel Markets
ModuFlex
The Scanacon ModuFlex is a highly efficient acid recovery system designed for a wide range of acid-based finishing processes in the stainless steel and titanium industries. It is specifically intended for hot and cold rolled and finished products, acid milling, etching of cast products, and single acid electrolytic processes.

Each modular unit has a maximum capacity of 500 L/hr and can be combined to handle larger flows ranging from 500 L/hr to 2,000 L/hr. This flexibility allows for a scalable solution to meet the specific needs of each application.

By implementing the ModuFlex, significant benefits can be achieved including improved productivity, reduced energy and resource consumption, decreased chemical use, improved health and safety conditions, improved economics, reduced environmental impact, and improved product quality. These benefits make the ModuFlex an ideal solution for the stainless steel market.
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